Primary ter add for internet connection in lpu or use ipconfig -all

Primary 172.19.2.254

Sec 172.19.2.252

Ter 172.19.2.250

DHCP client connection

Make changes in file

1. gedit /etc/sysconfig/network-scripts/ifcfg-eth0
2. gedit /etc/sysconfig/networking/devices/ifcfg-eth0
3. gedit /etc/sysconfig/networking/profiles/default/ifcfg-eth0

check\_link\_down()

{

return 1;

}